<?xml version='1.0' encoding='utf-8'?>
<?grc format='1' created='3.7.9'?>
<flow_graph>
  <timestamp>Fri Mar 18 13:57:31 2016</timestamp>
  <block>
    <key>options</key>
    <param>
      <key>author</key>
      <value></value>
    </param>
    <param>
      <key>window_size</key>
      <value>1720, 1080</value>
    </param>
    <param>
      <key>category</key>
      <value>Custom</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>description</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 8)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>generate_options</key>
      <value>qt_gui</value>
    </param>
    <param>
      <key>hier_block_src_path</key>
      <value>.:</value>
    </param>
    <param>
      <key>id</key>
      <value>debug_fsk_transceiver_uhd</value>
    </param>
    <param>
      <key>max_nouts</key>
      <value>0</value>
    </param>
    <param>
      <key>qt_qss_theme</key>
      <value></value>
    </param>
    <param>
      <key>realtime_scheduling</key>
      <value></value>
    </param>
    <param>
      <key>run_command</key>
      <value>{python} -u {filename}</value>
    </param>
    <param>
      <key>run_options</key>
      <value>prompt</value>
    </param>
    <param>
      <key>run</key>
      <value>True</value>
    </param>
    <param>
      <key>thread_safe_setters</key>
      <value></value>
    </param>
    <param>
      <key>title</key>
      <value></value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>FSK baud rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(808, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>baud_rate</value>
    </param>
    <param>
      <key>value</key>
      <value>9600</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>Decimation factor
for the RX after the
SDR received samples</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(272, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>decimation_rx</value>
    </param>
    <param>
      <key>value</key>
      <value>20</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>The FSK frequency deviation</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(648, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>deviation</value>
    </param>
    <param>
      <key>value</key>
      <value>3.9973e3</value>
    </param>
  </block>
  <block>
    <key>variable_qtgui_range</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>value</key>
      <value>20</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1384, 121)</value>
    </param>
    <param>
      <key>gui_hint</key>
      <value></value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>gain</value>
    </param>
    <param>
      <key>label</key>
      <value>Gain</value>
    </param>
    <param>
      <key>min_len</key>
      <value>200</value>
    </param>
    <param>
      <key>orient</key>
      <value>Qt.Horizontal</value>
    </param>
    <param>
      <key>start</key>
      <value>0</value>
    </param>
    <param>
      <key>step</key>
      <value>0.5</value>
    </param>
    <param>
      <key>stop</key>
      <value>30</value>
    </param>
    <param>
      <key>rangeType</key>
      <value>float</value>
    </param>
    <param>
      <key>widget</key>
      <value>counter_slider</value>
    </param>
  </block>
  <block>
    <key>variable_qtgui_range</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>value</key>
      <value>20</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1384, 9)</value>
    </param>
    <param>
      <key>gui_hint</key>
      <value></value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>gain_tx</value>
    </param>
    <param>
      <key>label</key>
      <value>Gain TX</value>
    </param>
    <param>
      <key>min_len</key>
      <value>200</value>
    </param>
    <param>
      <key>orient</key>
      <value>Qt.Horizontal</value>
    </param>
    <param>
      <key>start</key>
      <value>0</value>
    </param>
    <param>
      <key>step</key>
      <value>0.5</value>
    </param>
    <param>
      <key>stop</key>
      <value>70</value>
    </param>
    <param>
      <key>rangeType</key>
      <value>float</value>
    </param>
    <param>
      <key>widget</key>
      <value>counter_slider</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 589)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>gaussian_taps</value>
    </param>
    <param>
      <key>value</key>
      <value>filter.firdes.gaussian(1.0, samples_per_symbol_tx, 1.0, 4*samples_per_symbol_tx)</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 717)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>interp_taps</value>
    </param>
    <param>
      <key>value</key>
      <value>numpy.convolve(numpy.array(gaussian_taps), numpy.array(sq_wave))</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>To avoid the SDR carrier at the DC
we shift the LO a little further</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1200, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>lo_offset</value>
    </param>
    <param>
      <key>value</key>
      <value>100e3</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 517)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>modulation_index</value>
    </param>
    <param>
      <key>value</key>
      <value>deviation / (baud_rate / 2.0)</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>The RX center frequency
 of the system</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1056, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>rx_frequency</value>
    </param>
    <param>
      <key>value</key>
      <value>434e6</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 445)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samp_rate</value>
    </param>
    <param>
      <key>value</key>
      <value>samp_rate_rx/decimation_rx</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>SDR device 
TX sampling rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(408, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>value</key>
      <value>2e6</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>SDR device 
TX sampling rate</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(536, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>value</key>
      <value>2e6</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>Samples per FSK symbol.
Should be changed only for better
spectrum mask, or if the resampling
is too great and becomes a bottlneck.</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 117)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>samples_per_symbol_tx</value>
    </param>
    <param>
      <key>value</key>
      <value>4</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(8, 653)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>sq_wave</value>
    </param>
    <param>
      <key>value</key>
      <value>(1.0, ) * samples_per_symbol_tx</value>
    </param>
  </block>
  <block>
    <key>variable_low_pass_filter_taps</key>
    <param>
      <key>beta</key>
      <value>6.76</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>cutoff_freq</key>
      <value>20000</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1384, 242)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain</key>
      <value>1.0</value>
    </param>
    <param>
      <key>id</key>
      <value>taps</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>width</key>
      <value>60000</value>
    </param>
    <param>
      <key>win</key>
      <value>firdes.WIN_HAMMING</value>
    </param>
  </block>
  <block>
    <key>variable</key>
    <param>
      <key>comment</key>
      <value>The TX center frequency
 of the system</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(904, 13)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>tx_frequency</value>
    </param>
    <param>
      <key>value</key>
      <value>434e6</value>
    </param>
  </block>
  <block>
    <key>analog_frequency_modulator_fc</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1104, 524)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_frequency_modulator_fc_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>sensitivity</key>
      <value>(math.pi*modulation_index) / samples_per_symbol_tx</value>
    </param>
  </block>
  <block>
    <key>analog_quadrature_demod_cf</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(752, 252)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>gain</key>
      <value>(samp_rate / baud_rate)/(math.pi*modulation_index)</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_quadrature_demod_cf_0_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
  </block>
  <block>
    <key>analog_sig_source_x</key>
    <param>
      <key>amp</key>
      <value>1</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>freq</key>
      <value>lo_offset</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(912, 608)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>analog_sig_source_x_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>offset</key>
      <value>0</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>waveform</key>
      <value>analog.GR_COS_WAVE</value>
    </param>
  </block>
  <block>
    <key>blocks_multiply_xx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(776, 712)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>blocks_multiply_xx_0</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>num_inputs</key>
      <value>2</value>
    </param>
    <param>
      <key>vlen</key>
      <value>1</value>
    </param>
  </block>
  <block>
    <key>digital_clock_recovery_mm_xx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(904, 304)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>gain_mu</key>
      <value>0.175</value>
    </param>
    <param>
      <key>gain_omega</key>
      <value>0.25*0.175*0.175</value>
    </param>
    <param>
      <key>id</key>
      <value>digital_clock_recovery_mm_xx_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>mu</key>
      <value>0.5</value>
    </param>
    <param>
      <key>omega_relative_limit</key>
      <value>0.005</value>
    </param>
    <param>
      <key>omega</key>
      <value>samp_rate/baud_rate</value>
    </param>
    <param>
      <key>type</key>
      <value>float</value>
    </param>
  </block>
  <block>
    <key>freq_xlating_fir_filter_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>center_freq</key>
      <value>lo_offset</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>decim</key>
      <value>decimation_rx</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(456, 183)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>freq_xlating_fir_filter_xxx_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>taps</key>
      <value>taps</value>
    </param>
    <param>
      <key>type</key>
      <value>ccc</value>
    </param>
  </block>
  <block>
    <key>import</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1384, 420)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>import_0</value>
    </param>
    <param>
      <key>import</key>
      <value>import numpy</value>
    </param>
  </block>
  <block>
    <key>import</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1384, 372)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>import_0_0</value>
    </param>
    <param>
      <key>import</key>
      <value>import math</value>
    </param>
  </block>
  <block>
    <key>import</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1384, 468)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>import_0_1</value>
    </param>
    <param>
      <key>import</key>
      <value>from gnuradio import filter</value>
    </param>
  </block>
  <block>
    <key>interp_fir_filter_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(856, 517)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>interp_fir_filter_xxx_0</value>
    </param>
    <param>
      <key>interp</key>
      <value>samples_per_symbol_tx</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>samp_delay</key>
      <value>0</value>
    </param>
    <param>
      <key>taps</key>
      <value>interp_taps</value>
    </param>
    <param>
      <key>type</key>
      <value>fff</value>
    </param>
  </block>
  <block>
    <key>pfb_arb_resampler_xxx</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1080, 679)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>pfb_arb_resampler_xxx_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>nfilts</key>
      <value>32</value>
    </param>
    <param>
      <key>rrate</key>
      <value>samp_rate_tx / (baud_rate * samples_per_symbol_tx)</value>
    </param>
    <param>
      <key>samp_delay</key>
      <value>0</value>
    </param>
    <param>
      <key>atten</key>
      <value>60</value>
    </param>
    <param>
      <key>taps</key>
      <value>firdes.low_pass_2(32, 32, 0.8, 0.1, 60)</value>
    </param>
    <param>
      <key>type</key>
      <value>ccf</value>
    </param>
  </block>
  <block>
    <key>qtgui_freq_sink_x</key>
    <param>
      <key>autoscale</key>
      <value>False</value>
    </param>
    <param>
      <key>average</key>
      <value>1.0</value>
    </param>
    <param>
      <key>bw</key>
      <value>samp_rate_rx/10.0</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>fc</key>
      <value>0</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>ctrlpanel</key>
      <value>True</value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>0</value>
    </param>
    <param>
      <key>fftsize</key>
      <value>1024</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(1016, 174)</value>
    </param>
    <param>
      <key>gui_hint</key>
      <value></value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>grid</key>
      <value>True</value>
    </param>
    <param>
      <key>id</key>
      <value>qtgui_freq_sink_x_0</value>
    </param>
    <param>
      <key>legend</key>
      <value>True</value>
    </param>
    <param>
      <key>alpha1</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color1</key>
      <value>"blue"</value>
    </param>
    <param>
      <key>label1</key>
      <value></value>
    </param>
    <param>
      <key>width1</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha10</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color10</key>
      <value>"dark blue"</value>
    </param>
    <param>
      <key>label10</key>
      <value></value>
    </param>
    <param>
      <key>width10</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha2</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color2</key>
      <value>"red"</value>
    </param>
    <param>
      <key>label2</key>
      <value></value>
    </param>
    <param>
      <key>width2</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha3</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color3</key>
      <value>"green"</value>
    </param>
    <param>
      <key>label3</key>
      <value></value>
    </param>
    <param>
      <key>width3</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha4</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color4</key>
      <value>"black"</value>
    </param>
    <param>
      <key>label4</key>
      <value></value>
    </param>
    <param>
      <key>width4</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha5</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color5</key>
      <value>"cyan"</value>
    </param>
    <param>
      <key>label5</key>
      <value></value>
    </param>
    <param>
      <key>width5</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha6</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color6</key>
      <value>"magenta"</value>
    </param>
    <param>
      <key>label6</key>
      <value></value>
    </param>
    <param>
      <key>width6</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha7</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color7</key>
      <value>"yellow"</value>
    </param>
    <param>
      <key>label7</key>
      <value></value>
    </param>
    <param>
      <key>width7</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha8</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color8</key>
      <value>"dark red"</value>
    </param>
    <param>
      <key>label8</key>
      <value></value>
    </param>
    <param>
      <key>width8</key>
      <value>1</value>
    </param>
    <param>
      <key>alpha9</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color9</key>
      <value>"dark green"</value>
    </param>
    <param>
      <key>label9</key>
      <value></value>
    </param>
    <param>
      <key>width9</key>
      <value>1</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>name</key>
      <value>""</value>
    </param>
    <param>
      <key>nconnections</key>
      <value>1</value>
    </param>
    <param>
      <key>showports</key>
      <value>True</value>
    </param>
    <param>
      <key>freqhalf</key>
      <value>True</value>
    </param>
    <param>
      <key>tr_chan</key>
      <value>0</value>
    </param>
    <param>
      <key>tr_level</key>
      <value>0.0</value>
    </param>
    <param>
      <key>tr_mode</key>
      <value>qtgui.TRIG_MODE_FREE</value>
    </param>
    <param>
      <key>tr_tag</key>
      <value>""</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>update_time</key>
      <value>0.01</value>
    </param>
    <param>
      <key>wintype</key>
      <value>firdes.WIN_BLACKMAN_hARRIS</value>
    </param>
    <param>
      <key>ymax</key>
      <value>10</value>
    </param>
    <param>
      <key>ymin</key>
      <value>-140</value>
    </param>
  </block>
  <block>
    <key>qtgui_waterfall_sink_x</key>
    <param>
      <key>bw</key>
      <value>samp_rate_rx/10.0</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>fc</key>
      <value>0</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>0</value>
    </param>
    <param>
      <key>fftsize</key>
      <value>4096</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(808, 134)</value>
    </param>
    <param>
      <key>gui_hint</key>
      <value></value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>grid</key>
      <value>True</value>
    </param>
    <param>
      <key>id</key>
      <value>qtgui_waterfall_sink_x_0</value>
    </param>
    <param>
      <key>int_max</key>
      <value>10</value>
    </param>
    <param>
      <key>int_min</key>
      <value>-140</value>
    </param>
    <param>
      <key>legend</key>
      <value>True</value>
    </param>
    <param>
      <key>alpha1</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color1</key>
      <value>0</value>
    </param>
    <param>
      <key>label1</key>
      <value></value>
    </param>
    <param>
      <key>alpha10</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color10</key>
      <value>0</value>
    </param>
    <param>
      <key>label10</key>
      <value></value>
    </param>
    <param>
      <key>alpha2</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color2</key>
      <value>0</value>
    </param>
    <param>
      <key>label2</key>
      <value></value>
    </param>
    <param>
      <key>alpha3</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color3</key>
      <value>0</value>
    </param>
    <param>
      <key>label3</key>
      <value></value>
    </param>
    <param>
      <key>alpha4</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color4</key>
      <value>0</value>
    </param>
    <param>
      <key>label4</key>
      <value></value>
    </param>
    <param>
      <key>alpha5</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color5</key>
      <value>0</value>
    </param>
    <param>
      <key>label5</key>
      <value></value>
    </param>
    <param>
      <key>alpha6</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color6</key>
      <value>0</value>
    </param>
    <param>
      <key>label6</key>
      <value></value>
    </param>
    <param>
      <key>alpha7</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color7</key>
      <value>0</value>
    </param>
    <param>
      <key>label7</key>
      <value></value>
    </param>
    <param>
      <key>alpha8</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color8</key>
      <value>0</value>
    </param>
    <param>
      <key>label8</key>
      <value></value>
    </param>
    <param>
      <key>alpha9</key>
      <value>1.0</value>
    </param>
    <param>
      <key>color9</key>
      <value>0</value>
    </param>
    <param>
      <key>label9</key>
      <value></value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>name</key>
      <value>""</value>
    </param>
    <param>
      <key>nconnections</key>
      <value>1</value>
    </param>
    <param>
      <key>showports</key>
      <value>True</value>
    </param>
    <param>
      <key>freqhalf</key>
      <value>True</value>
    </param>
    <param>
      <key>type</key>
      <value>complex</value>
    </param>
    <param>
      <key>update_time</key>
      <value>0.05</value>
    </param>
    <param>
      <key>wintype</key>
      <value>firdes.WIN_BLACKMAN_hARRIS</value>
    </param>
  </block>
  <block>
    <key>satnogs_clear_text_msg_sink</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(288, 336)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_clear_text_msg_sink_0</value>
    </param>
  </block>
  <block>
    <key>satnogs_debug_msg_source</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>delay</key>
      <value>0.2</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(224, 510)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_debug_msg_source_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>msg</key>
      <value>"HELLO WORLD"</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>repeat</key>
      <value>True</value>
    </param>
  </block>
  <block>
    <key>satnogs_udp_msg_source</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value>The transmitter can also receive payloads 
from a UDP source. Use netcat or something
similar to produce dynamic payloads.</value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>True</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(216, 590)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_udp_msg_source_0</value>
    </param>
    <param>
      <key>addr</key>
      <value>"127.0.0.1"</value>
    </param>
    <param>
      <key>mtu</key>
      <value>1500</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>port</key>
      <value>16886</value>
    </param>
  </block>
  <block>
    <key>satnogs_upsat_fsk_frame_acquisition</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>check_crc</key>
      <value>True</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>preamble</key>
      <value>[0x33]*8 </value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(536, 304)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_upsat_fsk_frame_acquisition_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>sync_word</key>
      <value>[0x7A, 0x0E]</value>
    </param>
    <param>
      <key>manchester</key>
      <value>False</value>
    </param>
    <param>
      <key>whitening</key>
      <value>True</value>
    </param>
  </block>
  <block>
    <key>satnogs_upsat_fsk_frame_encoder</key>
    <param>
      <key>append_crc</key>
      <value>True</value>
    </param>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>preamble</key>
      <value>[0x33]*8 </value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(544, 482)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>satnogs_upsat_fsk_frame_encoder_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>settling_samples</key>
      <value>256</value>
    </param>
    <param>
      <key>msb_first</key>
      <value>True</value>
    </param>
    <param>
      <key>sync_word</key>
      <value>[0x7A, 0x0E]</value>
    </param>
    <param>
      <key>manchester</key>
      <value>False</value>
    </param>
    <param>
      <key>whitening</key>
      <value>True</value>
    </param>
  </block>
  <block>
    <key>uhd_usrp_sink</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>ant0</key>
      <value>TX/RX</value>
    </param>
    <param>
      <key>bw0</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>center_freq0</key>
      <value>tx_frequency - lo_offset</value>
    </param>
    <param>
      <key>norm_gain0</key>
      <value>False</value>
    </param>
    <param>
      <key>gain0</key>
      <value>gain_tx</value>
    </param>
    <param>
      <key>ant10</key>
      <value></value>
    </param>
    <param>
      <key>bw10</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq10</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain10</key>
      <value>False</value>
    </param>
    <param>
      <key>gain10</key>
      <value>0</value>
    </param>
    <param>
      <key>ant11</key>
      <value></value>
    </param>
    <param>
      <key>bw11</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq11</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain11</key>
      <value>False</value>
    </param>
    <param>
      <key>gain11</key>
      <value>0</value>
    </param>
    <param>
      <key>ant12</key>
      <value></value>
    </param>
    <param>
      <key>bw12</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq12</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain12</key>
      <value>False</value>
    </param>
    <param>
      <key>gain12</key>
      <value>0</value>
    </param>
    <param>
      <key>ant13</key>
      <value></value>
    </param>
    <param>
      <key>bw13</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq13</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain13</key>
      <value>False</value>
    </param>
    <param>
      <key>gain13</key>
      <value>0</value>
    </param>
    <param>
      <key>ant14</key>
      <value></value>
    </param>
    <param>
      <key>bw14</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq14</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain14</key>
      <value>False</value>
    </param>
    <param>
      <key>gain14</key>
      <value>0</value>
    </param>
    <param>
      <key>ant15</key>
      <value></value>
    </param>
    <param>
      <key>bw15</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq15</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain15</key>
      <value>False</value>
    </param>
    <param>
      <key>gain15</key>
      <value>0</value>
    </param>
    <param>
      <key>ant16</key>
      <value></value>
    </param>
    <param>
      <key>bw16</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq16</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain16</key>
      <value>False</value>
    </param>
    <param>
      <key>gain16</key>
      <value>0</value>
    </param>
    <param>
      <key>ant17</key>
      <value></value>
    </param>
    <param>
      <key>bw17</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq17</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain17</key>
      <value>False</value>
    </param>
    <param>
      <key>gain17</key>
      <value>0</value>
    </param>
    <param>
      <key>ant18</key>
      <value></value>
    </param>
    <param>
      <key>bw18</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq18</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain18</key>
      <value>False</value>
    </param>
    <param>
      <key>gain18</key>
      <value>0</value>
    </param>
    <param>
      <key>ant19</key>
      <value></value>
    </param>
    <param>
      <key>bw19</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq19</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain19</key>
      <value>False</value>
    </param>
    <param>
      <key>gain19</key>
      <value>0</value>
    </param>
    <param>
      <key>ant1</key>
      <value></value>
    </param>
    <param>
      <key>bw1</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq1</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain1</key>
      <value>False</value>
    </param>
    <param>
      <key>gain1</key>
      <value>0</value>
    </param>
    <param>
      <key>ant20</key>
      <value></value>
    </param>
    <param>
      <key>bw20</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq20</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain20</key>
      <value>False</value>
    </param>
    <param>
      <key>gain20</key>
      <value>0</value>
    </param>
    <param>
      <key>ant21</key>
      <value></value>
    </param>
    <param>
      <key>bw21</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq21</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain21</key>
      <value>False</value>
    </param>
    <param>
      <key>gain21</key>
      <value>0</value>
    </param>
    <param>
      <key>ant22</key>
      <value></value>
    </param>
    <param>
      <key>bw22</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq22</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain22</key>
      <value>False</value>
    </param>
    <param>
      <key>gain22</key>
      <value>0</value>
    </param>
    <param>
      <key>ant23</key>
      <value></value>
    </param>
    <param>
      <key>bw23</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq23</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain23</key>
      <value>False</value>
    </param>
    <param>
      <key>gain23</key>
      <value>0</value>
    </param>
    <param>
      <key>ant24</key>
      <value></value>
    </param>
    <param>
      <key>bw24</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq24</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain24</key>
      <value>False</value>
    </param>
    <param>
      <key>gain24</key>
      <value>0</value>
    </param>
    <param>
      <key>ant25</key>
      <value></value>
    </param>
    <param>
      <key>bw25</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq25</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain25</key>
      <value>False</value>
    </param>
    <param>
      <key>gain25</key>
      <value>0</value>
    </param>
    <param>
      <key>ant26</key>
      <value></value>
    </param>
    <param>
      <key>bw26</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq26</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain26</key>
      <value>False</value>
    </param>
    <param>
      <key>gain26</key>
      <value>0</value>
    </param>
    <param>
      <key>ant27</key>
      <value></value>
    </param>
    <param>
      <key>bw27</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq27</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain27</key>
      <value>False</value>
    </param>
    <param>
      <key>gain27</key>
      <value>0</value>
    </param>
    <param>
      <key>ant28</key>
      <value></value>
    </param>
    <param>
      <key>bw28</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq28</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain28</key>
      <value>False</value>
    </param>
    <param>
      <key>gain28</key>
      <value>0</value>
    </param>
    <param>
      <key>ant29</key>
      <value></value>
    </param>
    <param>
      <key>bw29</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq29</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain29</key>
      <value>False</value>
    </param>
    <param>
      <key>gain29</key>
      <value>0</value>
    </param>
    <param>
      <key>ant2</key>
      <value></value>
    </param>
    <param>
      <key>bw2</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq2</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain2</key>
      <value>False</value>
    </param>
    <param>
      <key>gain2</key>
      <value>0</value>
    </param>
    <param>
      <key>ant30</key>
      <value></value>
    </param>
    <param>
      <key>bw30</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq30</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain30</key>
      <value>False</value>
    </param>
    <param>
      <key>gain30</key>
      <value>0</value>
    </param>
    <param>
      <key>ant31</key>
      <value></value>
    </param>
    <param>
      <key>bw31</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq31</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain31</key>
      <value>False</value>
    </param>
    <param>
      <key>gain31</key>
      <value>0</value>
    </param>
    <param>
      <key>ant3</key>
      <value></value>
    </param>
    <param>
      <key>bw3</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq3</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain3</key>
      <value>False</value>
    </param>
    <param>
      <key>gain3</key>
      <value>0</value>
    </param>
    <param>
      <key>ant4</key>
      <value></value>
    </param>
    <param>
      <key>bw4</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq4</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain4</key>
      <value>False</value>
    </param>
    <param>
      <key>gain4</key>
      <value>0</value>
    </param>
    <param>
      <key>ant5</key>
      <value></value>
    </param>
    <param>
      <key>bw5</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq5</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain5</key>
      <value>False</value>
    </param>
    <param>
      <key>gain5</key>
      <value>0</value>
    </param>
    <param>
      <key>ant6</key>
      <value></value>
    </param>
    <param>
      <key>bw6</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq6</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain6</key>
      <value>False</value>
    </param>
    <param>
      <key>gain6</key>
      <value>0</value>
    </param>
    <param>
      <key>ant7</key>
      <value></value>
    </param>
    <param>
      <key>bw7</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq7</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain7</key>
      <value>False</value>
    </param>
    <param>
      <key>gain7</key>
      <value>0</value>
    </param>
    <param>
      <key>ant8</key>
      <value></value>
    </param>
    <param>
      <key>bw8</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq8</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain8</key>
      <value>False</value>
    </param>
    <param>
      <key>gain8</key>
      <value>0</value>
    </param>
    <param>
      <key>ant9</key>
      <value></value>
    </param>
    <param>
      <key>bw9</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq9</key>
      <value>0</value>
    </param>
    <param>
      <key>norm_gain9</key>
      <value>False</value>
    </param>
    <param>
      <key>gain9</key>
      <value>0</value>
    </param>
    <param>
      <key>clock_rate</key>
      <value>0.0</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>dev_addr</key>
      <value>""</value>
    </param>
    <param>
      <key>dev_args</key>
      <value>""</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(440, 705)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>180</value>
    </param>
    <param>
      <key>id</key>
      <value>uhd_usrp_sink_0</value>
    </param>
    <param>
      <key>type</key>
      <value>fc32</value>
    </param>
    <param>
      <key>clock_source0</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec0</key>
      <value></value>
    </param>
    <param>
      <key>time_source0</key>
      <value></value>
    </param>
    <param>
      <key>clock_source1</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec1</key>
      <value></value>
    </param>
    <param>
      <key>time_source1</key>
      <value></value>
    </param>
    <param>
      <key>clock_source2</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec2</key>
      <value></value>
    </param>
    <param>
      <key>time_source2</key>
      <value></value>
    </param>
    <param>
      <key>clock_source3</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec3</key>
      <value></value>
    </param>
    <param>
      <key>time_source3</key>
      <value></value>
    </param>
    <param>
      <key>clock_source4</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec4</key>
      <value></value>
    </param>
    <param>
      <key>time_source4</key>
      <value></value>
    </param>
    <param>
      <key>clock_source5</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec5</key>
      <value></value>
    </param>
    <param>
      <key>time_source5</key>
      <value></value>
    </param>
    <param>
      <key>clock_source6</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec6</key>
      <value></value>
    </param>
    <param>
      <key>time_source6</key>
      <value></value>
    </param>
    <param>
      <key>clock_source7</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec7</key>
      <value></value>
    </param>
    <param>
      <key>time_source7</key>
      <value></value>
    </param>
    <param>
      <key>nchan</key>
      <value>1</value>
    </param>
    <param>
      <key>num_mboards</key>
      <value>1</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_tx</value>
    </param>
    <param>
      <key>hide_cmd_port</key>
      <value>False</value>
    </param>
    <param>
      <key>stream_args</key>
      <value></value>
    </param>
    <param>
      <key>stream_chans</key>
      <value>[]</value>
    </param>
    <param>
      <key>sync</key>
      <value></value>
    </param>
    <param>
      <key>len_tag_name</key>
      <value></value>
    </param>
    <param>
      <key>otw</key>
      <value></value>
    </param>
  </block>
  <block>
    <key>uhd_usrp_source</key>
    <param>
      <key>alias</key>
      <value></value>
    </param>
    <param>
      <key>ant0</key>
      <value>RX2</value>
    </param>
    <param>
      <key>bw0</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>center_freq0</key>
      <value>rx_frequency - lo_offset</value>
    </param>
    <param>
      <key>dc_offs_enb0</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb0</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain0</key>
      <value>False</value>
    </param>
    <param>
      <key>gain0</key>
      <value>gain</value>
    </param>
    <param>
      <key>ant10</key>
      <value></value>
    </param>
    <param>
      <key>bw10</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq10</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb10</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb10</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain10</key>
      <value>False</value>
    </param>
    <param>
      <key>gain10</key>
      <value>0</value>
    </param>
    <param>
      <key>ant11</key>
      <value></value>
    </param>
    <param>
      <key>bw11</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq11</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb11</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb11</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain11</key>
      <value>False</value>
    </param>
    <param>
      <key>gain11</key>
      <value>0</value>
    </param>
    <param>
      <key>ant12</key>
      <value></value>
    </param>
    <param>
      <key>bw12</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq12</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb12</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb12</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain12</key>
      <value>False</value>
    </param>
    <param>
      <key>gain12</key>
      <value>0</value>
    </param>
    <param>
      <key>ant13</key>
      <value></value>
    </param>
    <param>
      <key>bw13</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq13</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb13</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb13</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain13</key>
      <value>False</value>
    </param>
    <param>
      <key>gain13</key>
      <value>0</value>
    </param>
    <param>
      <key>ant14</key>
      <value></value>
    </param>
    <param>
      <key>bw14</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq14</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb14</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb14</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain14</key>
      <value>False</value>
    </param>
    <param>
      <key>gain14</key>
      <value>0</value>
    </param>
    <param>
      <key>ant15</key>
      <value></value>
    </param>
    <param>
      <key>bw15</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq15</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb15</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb15</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain15</key>
      <value>False</value>
    </param>
    <param>
      <key>gain15</key>
      <value>0</value>
    </param>
    <param>
      <key>ant16</key>
      <value></value>
    </param>
    <param>
      <key>bw16</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq16</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb16</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb16</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain16</key>
      <value>False</value>
    </param>
    <param>
      <key>gain16</key>
      <value>0</value>
    </param>
    <param>
      <key>ant17</key>
      <value></value>
    </param>
    <param>
      <key>bw17</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq17</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb17</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb17</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain17</key>
      <value>False</value>
    </param>
    <param>
      <key>gain17</key>
      <value>0</value>
    </param>
    <param>
      <key>ant18</key>
      <value></value>
    </param>
    <param>
      <key>bw18</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq18</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb18</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb18</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain18</key>
      <value>False</value>
    </param>
    <param>
      <key>gain18</key>
      <value>0</value>
    </param>
    <param>
      <key>ant19</key>
      <value></value>
    </param>
    <param>
      <key>bw19</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq19</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb19</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb19</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain19</key>
      <value>False</value>
    </param>
    <param>
      <key>gain19</key>
      <value>0</value>
    </param>
    <param>
      <key>ant1</key>
      <value></value>
    </param>
    <param>
      <key>bw1</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq1</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb1</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb1</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain1</key>
      <value>False</value>
    </param>
    <param>
      <key>gain1</key>
      <value>0</value>
    </param>
    <param>
      <key>ant20</key>
      <value></value>
    </param>
    <param>
      <key>bw20</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq20</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb20</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb20</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain20</key>
      <value>False</value>
    </param>
    <param>
      <key>gain20</key>
      <value>0</value>
    </param>
    <param>
      <key>ant21</key>
      <value></value>
    </param>
    <param>
      <key>bw21</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq21</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb21</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb21</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain21</key>
      <value>False</value>
    </param>
    <param>
      <key>gain21</key>
      <value>0</value>
    </param>
    <param>
      <key>ant22</key>
      <value></value>
    </param>
    <param>
      <key>bw22</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq22</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb22</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb22</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain22</key>
      <value>False</value>
    </param>
    <param>
      <key>gain22</key>
      <value>0</value>
    </param>
    <param>
      <key>ant23</key>
      <value></value>
    </param>
    <param>
      <key>bw23</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq23</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb23</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb23</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain23</key>
      <value>False</value>
    </param>
    <param>
      <key>gain23</key>
      <value>0</value>
    </param>
    <param>
      <key>ant24</key>
      <value></value>
    </param>
    <param>
      <key>bw24</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq24</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb24</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb24</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain24</key>
      <value>False</value>
    </param>
    <param>
      <key>gain24</key>
      <value>0</value>
    </param>
    <param>
      <key>ant25</key>
      <value></value>
    </param>
    <param>
      <key>bw25</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq25</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb25</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb25</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain25</key>
      <value>False</value>
    </param>
    <param>
      <key>gain25</key>
      <value>0</value>
    </param>
    <param>
      <key>ant26</key>
      <value></value>
    </param>
    <param>
      <key>bw26</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq26</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb26</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb26</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain26</key>
      <value>False</value>
    </param>
    <param>
      <key>gain26</key>
      <value>0</value>
    </param>
    <param>
      <key>ant27</key>
      <value></value>
    </param>
    <param>
      <key>bw27</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq27</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb27</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb27</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain27</key>
      <value>False</value>
    </param>
    <param>
      <key>gain27</key>
      <value>0</value>
    </param>
    <param>
      <key>ant28</key>
      <value></value>
    </param>
    <param>
      <key>bw28</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq28</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb28</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb28</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain28</key>
      <value>False</value>
    </param>
    <param>
      <key>gain28</key>
      <value>0</value>
    </param>
    <param>
      <key>ant29</key>
      <value></value>
    </param>
    <param>
      <key>bw29</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq29</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb29</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb29</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain29</key>
      <value>False</value>
    </param>
    <param>
      <key>gain29</key>
      <value>0</value>
    </param>
    <param>
      <key>ant2</key>
      <value></value>
    </param>
    <param>
      <key>bw2</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq2</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb2</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb2</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain2</key>
      <value>False</value>
    </param>
    <param>
      <key>gain2</key>
      <value>0</value>
    </param>
    <param>
      <key>ant30</key>
      <value></value>
    </param>
    <param>
      <key>bw30</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq30</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb30</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb30</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain30</key>
      <value>False</value>
    </param>
    <param>
      <key>gain30</key>
      <value>0</value>
    </param>
    <param>
      <key>ant31</key>
      <value></value>
    </param>
    <param>
      <key>bw31</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq31</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb31</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb31</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain31</key>
      <value>False</value>
    </param>
    <param>
      <key>gain31</key>
      <value>0</value>
    </param>
    <param>
      <key>ant3</key>
      <value></value>
    </param>
    <param>
      <key>bw3</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq3</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb3</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb3</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain3</key>
      <value>False</value>
    </param>
    <param>
      <key>gain3</key>
      <value>0</value>
    </param>
    <param>
      <key>ant4</key>
      <value></value>
    </param>
    <param>
      <key>bw4</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq4</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb4</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb4</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain4</key>
      <value>False</value>
    </param>
    <param>
      <key>gain4</key>
      <value>0</value>
    </param>
    <param>
      <key>ant5</key>
      <value></value>
    </param>
    <param>
      <key>bw5</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq5</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb5</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb5</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain5</key>
      <value>False</value>
    </param>
    <param>
      <key>gain5</key>
      <value>0</value>
    </param>
    <param>
      <key>ant6</key>
      <value></value>
    </param>
    <param>
      <key>bw6</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq6</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb6</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb6</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain6</key>
      <value>False</value>
    </param>
    <param>
      <key>gain6</key>
      <value>0</value>
    </param>
    <param>
      <key>ant7</key>
      <value></value>
    </param>
    <param>
      <key>bw7</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq7</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb7</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb7</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain7</key>
      <value>False</value>
    </param>
    <param>
      <key>gain7</key>
      <value>0</value>
    </param>
    <param>
      <key>ant8</key>
      <value></value>
    </param>
    <param>
      <key>bw8</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq8</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb8</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb8</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain8</key>
      <value>False</value>
    </param>
    <param>
      <key>gain8</key>
      <value>0</value>
    </param>
    <param>
      <key>ant9</key>
      <value></value>
    </param>
    <param>
      <key>bw9</key>
      <value>0</value>
    </param>
    <param>
      <key>center_freq9</key>
      <value>0</value>
    </param>
    <param>
      <key>dc_offs_enb9</key>
      <value>""</value>
    </param>
    <param>
      <key>iq_imbal_enb9</key>
      <value>""</value>
    </param>
    <param>
      <key>norm_gain9</key>
      <value>False</value>
    </param>
    <param>
      <key>gain9</key>
      <value>0</value>
    </param>
    <param>
      <key>clock_rate</key>
      <value>0.0</value>
    </param>
    <param>
      <key>comment</key>
      <value></value>
    </param>
    <param>
      <key>affinity</key>
      <value></value>
    </param>
    <param>
      <key>dev_addr</key>
      <value>""</value>
    </param>
    <param>
      <key>dev_args</key>
      <value>""</value>
    </param>
    <param>
      <key>_enabled</key>
      <value>1</value>
    </param>
    <param>
      <key>_coordinate</key>
      <value>(248, 160)</value>
    </param>
    <param>
      <key>_rotation</key>
      <value>0</value>
    </param>
    <param>
      <key>id</key>
      <value>uhd_usrp_source_0</value>
    </param>
    <param>
      <key>maxoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>clock_source0</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec0</key>
      <value></value>
    </param>
    <param>
      <key>time_source0</key>
      <value></value>
    </param>
    <param>
      <key>clock_source1</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec1</key>
      <value></value>
    </param>
    <param>
      <key>time_source1</key>
      <value></value>
    </param>
    <param>
      <key>clock_source2</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec2</key>
      <value></value>
    </param>
    <param>
      <key>time_source2</key>
      <value></value>
    </param>
    <param>
      <key>clock_source3</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec3</key>
      <value></value>
    </param>
    <param>
      <key>time_source3</key>
      <value></value>
    </param>
    <param>
      <key>clock_source4</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec4</key>
      <value></value>
    </param>
    <param>
      <key>time_source4</key>
      <value></value>
    </param>
    <param>
      <key>clock_source5</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec5</key>
      <value></value>
    </param>
    <param>
      <key>time_source5</key>
      <value></value>
    </param>
    <param>
      <key>clock_source6</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec6</key>
      <value></value>
    </param>
    <param>
      <key>time_source6</key>
      <value></value>
    </param>
    <param>
      <key>clock_source7</key>
      <value></value>
    </param>
    <param>
      <key>sd_spec7</key>
      <value></value>
    </param>
    <param>
      <key>time_source7</key>
      <value></value>
    </param>
    <param>
      <key>minoutbuf</key>
      <value>0</value>
    </param>
    <param>
      <key>nchan</key>
      <value>1</value>
    </param>
    <param>
      <key>num_mboards</key>
      <value>1</value>
    </param>
    <param>
      <key>type</key>
      <value>fc32</value>
    </param>
    <param>
      <key>samp_rate</key>
      <value>samp_rate_rx</value>
    </param>
    <param>
      <key>hide_cmd_port</key>
      <value>False</value>
    </param>
    <param>
      <key>stream_args</key>
      <value></value>
    </param>
    <param>
      <key>stream_chans</key>
      <value>[]</value>
    </param>
    <param>
      <key>sync</key>
      <value></value>
    </param>
    <param>
      <key>otw</key>
      <value></value>
    </param>
  </block>
  <connection>
    <source_block_id>analog_frequency_modulator_fc_0</source_block_id>
    <sink_block_id>pfb_arb_resampler_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>analog_quadrature_demod_cf_0_0</source_block_id>
    <sink_block_id>digital_clock_recovery_mm_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>analog_sig_source_x_0</source_block_id>
    <sink_block_id>blocks_multiply_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>1</sink_key>
  </connection>
  <connection>
    <source_block_id>blocks_multiply_xx_0</source_block_id>
    <sink_block_id>uhd_usrp_sink_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>digital_clock_recovery_mm_xx_0</source_block_id>
    <sink_block_id>satnogs_upsat_fsk_frame_acquisition_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>freq_xlating_fir_filter_xxx_0</source_block_id>
    <sink_block_id>analog_quadrature_demod_cf_0_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>freq_xlating_fir_filter_xxx_0</source_block_id>
    <sink_block_id>qtgui_freq_sink_x_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>freq_xlating_fir_filter_xxx_0</source_block_id>
    <sink_block_id>qtgui_waterfall_sink_x_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>interp_fir_filter_xxx_0</source_block_id>
    <sink_block_id>analog_frequency_modulator_fc_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>pfb_arb_resampler_xxx_0</source_block_id>
    <sink_block_id>blocks_multiply_xx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_debug_msg_source_0</source_block_id>
    <sink_block_id>satnogs_upsat_fsk_frame_encoder_0</sink_block_id>
    <source_key>msg</source_key>
    <sink_key>pdu</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_udp_msg_source_0</source_block_id>
    <sink_block_id>satnogs_upsat_fsk_frame_encoder_0</sink_block_id>
    <source_key>msg</source_key>
    <sink_key>pdu</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_upsat_fsk_frame_acquisition_0</source_block_id>
    <sink_block_id>satnogs_clear_text_msg_sink_0</sink_block_id>
    <source_key>pdu</source_key>
    <sink_key>in</sink_key>
  </connection>
  <connection>
    <source_block_id>satnogs_upsat_fsk_frame_encoder_0</source_block_id>
    <sink_block_id>interp_fir_filter_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
  <connection>
    <source_block_id>uhd_usrp_source_0</source_block_id>
    <sink_block_id>freq_xlating_fir_filter_xxx_0</sink_block_id>
    <source_key>0</source_key>
    <sink_key>0</sink_key>
  </connection>
</flow_graph>
