(export (version D)
  (design
    (source /home/sebastian/projects/7segment_timer/boards/levelshifter/leveshifterboard.sch)
    (date "Tue 19 Aug 2014 11:19:38 PM CEST")
    (tool "eeschema (2013-may-18)-stable"))
  (components
    (comp (ref C4)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA2601))
    (comp (ref C3)
      (value 10uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA2602))
    (comp (ref C6)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA2603))
    (comp (ref C5)
      (value 10uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA2604))
    (comp (ref R10)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA2609))
    (comp (ref D4)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA260A))
    (comp (ref R9)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA260C))
    (comp (ref D2)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA260D))
    (comp (ref D3)
      (value BAT42W)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA260F))
    (comp (ref U4)
      (value TS2937)
      (libsource (lib ts2937) (part TS2937))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA2610))
    (comp (ref P1)
      (value CONN_2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA264E))
    (comp (ref J1)
      (value RJ45)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 52EA29B9))
    (comp (ref U1)
      (value LM358)
      (libsource (lib linear) (part LM358))
      (sheetpath (names /) (tstamps /))
      (tstamp 530A359C))
    (comp (ref R5)
      (value 0.05)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 530A35B5))
    (comp (ref F1)
      (value FUSE)
      (libsource (lib device) (part FUSE))
      (sheetpath (names /) (tstamps /))
      (tstamp 530A3B07))
    (comp (ref R1)
      (value 10k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 530A40D1))
    (comp (ref R2)
      (value 90k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 530A4269))
    (comp (ref RV1)
      (value POT)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 530A46D9))
    (comp (ref U2)
      (value SN74LVC1G74)
      (libsource (lib sn74lvc1g74) (part SN74LVC1G74))
      (sheetpath (names /) (tstamps /))
      (tstamp 530DC723))
    (comp (ref SW1)
      (value SW_PUSH)
      (libsource (lib device) (part SW_PUSH))
      (sheetpath (names /) (tstamps /))
      (tstamp 530DCE0D))
    (comp (ref R8)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 530DCF8E))
    (comp (ref R6)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 530DD3FA))
    (comp (ref R3)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 530DD544))
    (comp (ref R7)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 530DD88F))
    (comp (ref D1)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 530DD89E))
    (comp (ref U3)
      (value 74HCT125)
      (libsource (lib 74hct125) (part 74HCT125))
      (sheetpath (names /) (tstamps /))
      (tstamp 530E5BAD))
    (comp (ref C2)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 530E62FF))
    (comp (ref R4)
      (value 100k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53135149))
    (comp (ref C1)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 53135158))
    (comp (ref C7)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5315FBCE))
    (comp (ref R12)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53160BB6))
    (comp (ref P2)
      (value CONN_7)
      (libsource (lib conn) (part CONN_7))
      (sheetpath (names /) (tstamps /))
      (tstamp 53160F8F))
    (comp (ref R11)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5316122F))
    (comp (ref Q2)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 53174CCD))
    (comp (ref Q1)
      (value IRLR110)
      (libsource (lib irlr110) (part IRLR110))
      (sheetpath (names /) (tstamps /))
      (tstamp 53174CDC))
    (comp (ref D5)
      (value ZENER_5.6V)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3BB95))
    (comp (ref D6)
      (value ZENER_5.6V)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3BBA2))
    (comp (ref D7)
      (value ZENER_5.6V)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3BBA8))
    (comp (ref D8)
      (value ZENER_5.6V)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3BBAE))
    (comp (ref R13)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3C2AF))
    (comp (ref R14)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3C2BC))
    (comp (ref R15)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3C2C2))
    (comp (ref R16)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53F3C2C8)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part FUSE)
      (fields
        (field (name Reference) F)
        (field (name Value) FUSE)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part POT)
      (description Potentionmetre)
      (fields
        (field (name Reference) RV)
        (field (name Value) POT)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part SW_PUSH)
      (description "Push Button")
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_PUSH)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part ZENER)
      (description "Diode zener")
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) ZENER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib conn) (part CONN_7)
      (description "Symbole general pour connexions")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_7)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))))
    (libpart (lib conn) (part RJ45)
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name SHIELD) (type passive))))
    (libpart (lib linear) (part LM358)
      (description "Dual Op amp (low power)")
      (docs ns/lm158.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) LM358))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name V+) (type power_in))))
    (libpart (lib sn74lvc1g74) (part SN74LVC1G74)
      (fields
        (field (name Reference) U)
        (field (name Value) SN74LVC1G74)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name CLK) (type input))
        (pin (num 2) (name D) (type input))
        (pin (num 3) (name notQ) (type input))
        (pin (num 4) (name GND) (type input))
        (pin (num 5) (name Q) (type input))
        (pin (num 6) (name CLR) (type input))
        (pin (num 7) (name PRE) (type input))
        (pin (num 8) (name Vcc) (type input))))
    (libpart (lib 74hct125) (part 74HCT125)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HCT125)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name OE1) (type input))
        (pin (num 2) (name 1A) (type input))
        (pin (num 3) (name Y1) (type input))
        (pin (num 4) (name OE2) (type input))
        (pin (num 5) (name 2A) (type input))
        (pin (num 6) (name Y2) (type input))
        (pin (num 7) (name GND) (type input))
        (pin (num 8) (name Y3) (type input))
        (pin (num 9) (name 3A) (type input))
        (pin (num 10) (name OE3) (type input))
        (pin (num 11) (name Y4) (type input))
        (pin (num 12) (name 4A) (type input))
        (pin (num 13) (name OE4) (type input))
        (pin (num 14) (name Vcc) (type input))))
    (libpart (lib ts2937) (part TS2937)
      (fields
        (field (name Reference) U)
        (field (name Value) TS2937)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VI) (type input))
        (pin (num 2) (name GND) (type input))
        (pin (num 3) (name VO) (type power_out))))
    (libpart (lib nds355) (part NDS355)
      (fields
        (field (name Reference) Q)
        (field (name Value) NDS355)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib irlr110) (part IRLR110)
      (fields
        (field (name Reference) Q)
        (field (name Value) IRLR110)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical linear)
      (uri /usr/share/kicad/library/linear.lib))
    (library (logical ts2937)
      (uri ../lib/ts2937.lib))
    (library (logical sn74lvc1g74)
      (uri ../lib/sn74lvc1g74.lib))
    (library (logical nds355)
      (uri ../lib/nds355.lib))
    (library (logical 74hct125)
      (uri ../lib/74hct125.lib))
    (library (logical irlr110)
      (uri ../lib/irlr110.lib)))
  (nets
    (net (code 1) (name +5V)
      (node (ref U1) (pin 8))
      (node (ref D3) (pin 1))
      (node (ref U4) (pin 3))
      (node (ref C6) (pin 1))
      (node (ref R10) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref RV1) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref U3) (pin 14))
      (node (ref C2) (pin 1)))
    (net (code 2) (name BusOff)
      (node (ref R11) (pin 1))
      (node (ref U3) (pin 4))
      (node (ref U3) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref U3) (pin 10))
      (node (ref U3) (pin 13))
      (node (ref R7) (pin 1)))
    (net (code 3) (name "")
      (node (ref R4) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 4) (name "")
      (node (ref R8) (pin 1))
      (node (ref SW1) (pin 1))
      (node (ref U2) (pin 6)))
    (net (code 5) (name "")
      (node (ref R7) (pin 2))
      (node (ref D1) (pin 1)))
    (net (code 6) (name "")
      (node (ref U1) (pin 5))
      (node (ref RV1) (pin 2)))
    (net (code 7) (name Sense)
      (node (ref U1) (pin 3))
      (node (ref J1) (pin 9))
      (node (ref J1) (pin 8))
      (node (ref R5) (pin 1))
      (node (ref J1) (pin 6)))
    (net (code 8) (name "")
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 9) (name +24V)
      (node (ref R9) (pin 1))
      (node (ref D3) (pin 2))
      (node (ref U4) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref F1) (pin 2))
      (node (ref Q1) (pin 2)))
    (net (code 10) (name "")
      (node (ref F1) (pin 1))
      (node (ref P1) (pin 2)))
    (net (code 11) (name GND)
      (node (ref R5) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref RV1) (pin 3))
      (node (ref R1) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref U2) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref D4) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref Q2) (pin 3))
      (node (ref D5) (pin 1))
      (node (ref D6) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref D8) (pin 1))
      (node (ref U3) (pin 7))
      (node (ref U1) (pin 4))
      (node (ref P2) (pin 7)))
    (net (code 12) (name Shutdown)
      (node (ref U2) (pin 7))
      (node (ref R6) (pin 2))
      (node (ref U1) (pin 7)))
    (net (code 13) (name PowerOn)
      (node (ref Q1) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref R3) (pin 2)))
    (net (code 14) (name "")
      (node (ref U3) (pin 11))
      (node (ref R16) (pin 1))
      (node (ref D8) (pin 2)))
    (net (code 15) (name "")
      (node (ref D7) (pin 2))
      (node (ref U3) (pin 8))
      (node (ref R15) (pin 1)))
    (net (code 16) (name "")
      (node (ref D6) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref U3) (pin 6)))
    (net (code 17) (name "")
      (node (ref D5) (pin 2))
      (node (ref R13) (pin 1))
      (node (ref U3) (pin 3)))
    (net (code 18) (name "")
      (node (ref Q2) (pin 1))
      (node (ref R11) (pin 2)))
    (net (code 19) (name Reset)
      (node (ref R16) (pin 2))
      (node (ref J1) (pin 7)))
    (net (code 20) (name Data_Out)
      (node (ref R15) (pin 2))
      (node (ref J1) (pin 5)))
    (net (code 21) (name Enable)
      (node (ref J1) (pin 3))
      (node (ref R14) (pin 2)))
    (net (code 22) (name Clock)
      (node (ref R13) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 23) (name "")
      (node (ref Q2) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref P2) (pin 6)))
    (net (code 24) (name "")
      (node (ref C1) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 25) (name +3.3V)
      (node (ref R12) (pin 1))
      (node (ref P2) (pin 1)))
    (net (code 26) (name 3.3_Reset)
      (node (ref P2) (pin 5))
      (node (ref U3) (pin 12)))
    (net (code 27) (name 3.3_Enable)
      (node (ref U3) (pin 5))
      (node (ref P2) (pin 4)))
    (net (code 28) (name 3.3_Data_Out)
      (node (ref P2) (pin 3))
      (node (ref U3) (pin 9)))
    (net (code 29) (name 3.3_Clock)
      (node (ref U3) (pin 2))
      (node (ref P2) (pin 2)))
    (net (code 30) (name "")
      (node (ref D4) (pin 1))
      (node (ref R10) (pin 2)))
    (net (code 31) (name "")
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref Q1) (pin 3)))
    (net (code 32) (name "")
      (node (ref R9) (pin 2))
      (node (ref D2) (pin 1)))))