(export (version D)
  (design
    (source /home/sebastian/projects/LipoGuard/lipoguard.sch)
    (date "Wed 05 Oct 2016 11:28:54 PM CEST")
    (tool "Eeschema 4.0.4-stable")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source lipoguard.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value BTS6143)
      (footprint to252-5:TO252-5L)
      (libsource (lib bts6143) (part BTS6143))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E2D89A))
    (comp (ref R3)
      (value R)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E2E0BA))
    (comp (ref P2)
      (value CONN_2)
      (footprint connect:bornier2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E2E27C))
    (comp (ref R2)
      (value R)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E2E5E3))
    (comp (ref D2)
      (value LED)
      (footprint libcms:SM0603)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E2E629))
    (comp (ref R1)
      (value R)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E2F4FB))
    (comp (ref D1)
      (value LED)
      (footprint libcms:SM0603)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E2F7BC))
    (comp (ref P1)
      (value CONN_2)
      (footprint connect:bornier2)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 57E30469))
    (comp (ref Q1)
      (value "BC 850C")
      (footprint misc:sot23BEC)
      (libsource (lib device) (part NPN))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F2671F))
    (comp (ref R4)
      (value 4.7k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F269B7))
    (comp (ref C1)
      (value 100nf)
      (footprint libcms:SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F3D205))
    (comp (ref RV1)
      (value 5k)
      (footprint misc:trimmer1)
      (libsource (lib device) (part POT))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F26A5C))
    (comp (ref R5)
      (value 10k)
      (footprint libcms:SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 57F56FF8)))
  (libparts
    (libpart (lib bts6143) (part BTS6143)
      (fields
        (field (name Reference) U)
        (field (name Value) BTS6143))
      (pins
        (pin (num 1) (name Out) (type input))
        (pin (num 2) (name In) (type input))
        (pin (num 3) (name Vbb) (type input))
        (pin (num 4) (name Is) (type input))
        (pin (num 5) (name Out) (type input))))
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part NPN)
      (docs transistors/bipolar/*.*)
      (fields
        (field (name Reference) Q)
        (field (name Value) NPN))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type input))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib device) (part POT)
      (description Potentionmetre)
      (fields
        (field (name Reference) RV)
        (field (name Value) POT))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical bts6143)
      (uri /home/sebastian/projects/LipoGuard/lib/bts6143.lib)))
  (nets
    (net (code 1) (name VCC)
      (node (ref P1) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 3)))
    (net (code 2) (name GND)
      (node (ref P2) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref D2) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref RV1) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref C1) (pin 2)))
    (net (code 3) (name "Net-(Q1-Pad3)")
      (node (ref U1) (pin 2))
      (node (ref Q1) (pin 3)))
    (net (code 4) (name "Net-(Q1-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref Q1) (pin 2)))
    (net (code 5) (name "Net-(R5-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref RV1) (pin 3)))
    (net (code 6) (name "Net-(C1-Pad1)")
      (node (ref RV1) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 7) (name "Net-(D1-Pad1)")
      (node (ref D1) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 8) (name "Net-(R3-Pad1)")
      (node (ref U1) (pin 4))
      (node (ref R3) (pin 1)))
    (net (code 9) (name "Net-(D2-Pad1)")
      (node (ref D2) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 10) (name "Net-(P2-Pad2)")
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref R2) (pin 1))
      (node (ref P2) (pin 2)))))