Cmp-Mod V01 Created by CvPcb (2012-12-10 BZR 3844)-stable date = Thu 13 Dec 2012 04:00:08 PM CET

BeginCmp
TimeStamp = /5069B992;
Reference = C1;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069B6DA;
Reference = C2;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069B6D1;
Reference = C3;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069B4C5;
Reference = C4;
ValeurCmp = 22pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069B4CA;
Reference = C5;
ValeurCmp = 22pF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4AE4A;
Reference = C6;
ValeurCmp = 10uF_tantal;
IdModule  = c_elec_5x5.3;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D91CA;
Reference = C7;
ValeurCmp = 4,7uF_tantal;
IdModule  = c_elec_4x4.5;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D9131;
Reference = C8;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D902E;
Reference = C9;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D979D;
Reference = C10;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4AE59;
Reference = C11;
ValeurCmp = 10uF_tantal;
IdModule  = c_elec_5x5.3;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4AE68;
Reference = C12;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4B496;
Reference = D1;
ValeurCmp = LED;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4BF42;
Reference = D2;
ValeurCmp = BAT42W;
IdModule  = sod123;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D9AAB;
Reference = D6;
ValeurCmp = LED;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D9ABA;
Reference = D7;
ValeurCmp = LED;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069B452;
Reference = IC1;
ValeurCmp = ATMEGA8-P;
IdModule  = DIP-28__300_ELL;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D8ECA;
Reference = J1;
ValeurCmp = USB;
IdModule  = conn_usb_B_mini_smd;
EndCmp

BeginCmp
TimeStamp = /5069B88A;
Reference = JP1;
ValeurCmp = JUMPER;
IdModule  = SIL-2;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/5069B18D;
Reference = JP2;
ValeurCmp = JUMPER;
IdModule  = SIL-2;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/5069B17A;
Reference = JP3;
ValeurCmp = JUMPER;
IdModule  = SIL-2;
EndCmp

BeginCmp
TimeStamp = /5069CEA2;
Reference = K1;
ValeurCmp = CONN_3;
IdModule  = SIL-3;
EndCmp

BeginCmp
TimeStamp = /5069D40C;
Reference = K2;
ValeurCmp = CONN_3;
IdModule  = SIL-3;
EndCmp

BeginCmp
TimeStamp = /5069D3E5;
Reference = K3;
ValeurCmp = CONN_3;
IdModule  = SIL-3;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/5069B154;
Reference = L1;
ValeurCmp = INDUCTOR;
IdModule  = SM0805;
EndCmp

BeginCmp
TimeStamp = /5069CE7E;
Reference = P1;
ValeurCmp = CONN_6;
IdModule  = SIL-6;
EndCmp

BeginCmp
TimeStamp = /5069CE8A;
Reference = P2;
ValeurCmp = CONN_6;
IdModule  = SIL-6;
EndCmp

BeginCmp
TimeStamp = /5069D130;
Reference = P3;
ValeurCmp = CONN_6;
IdModule  = SIL-6;
EndCmp

BeginCmp
TimeStamp = /5069D139;
Reference = P4;
ValeurCmp = CONN_6;
IdModule  = SIL-6;
EndCmp

BeginCmp
TimeStamp = /5069CE9B;
Reference = P5;
ValeurCmp = CONN_5;
IdModule  = SIL-5;
EndCmp

BeginCmp
TimeStamp = /5069D2A4;
Reference = P6;
ValeurCmp = CONN_6;
IdModule  = SIL-6;
EndCmp

BeginCmp
TimeStamp = /5069D329;
Reference = P7;
ValeurCmp = CONN_5;
IdModule  = SIL-5;
EndCmp

BeginCmp
TimeStamp = /5069D2A3;
Reference = P8;
ValeurCmp = CONN_6;
IdModule  = SIL-6;
EndCmp

BeginCmp
TimeStamp = /5069D32F;
Reference = P9;
ValeurCmp = CONN_5;
IdModule  = SIL-5;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4B3A1;
Reference = P10;
ValeurCmp = CONN_2;
IdModule  = bornier2;
EndCmp

BeginCmp
TimeStamp = /50C6F989;
Reference = P11;
ValeurCmp = CONN_3X2;
IdModule  = pin_array_3x2;
EndCmp

BeginCmp
TimeStamp = /5069BA5E;
Reference = R1;
ValeurCmp = 10k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4B487;
Reference = R2;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D95ED;
Reference = R8;
ValeurCmp = 4,7k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D95FC;
Reference = R9;
ValeurCmp = 10k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D991D;
Reference = R10;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D992C;
Reference = R11;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /5069B78F;
Reference = SW1;
ValeurCmp = SW_PUSH;
IdModule  = SW_PUSH_SMALL;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/4F9D8EBB;
Reference = U1;
ValeurCmp = FT232RL;
IdModule  = SSOP28;
EndCmp

BeginCmp
TimeStamp = /5069AFCC/50C4BBB3;
Reference = U2;
ValeurCmp = LM1117;
IdModule  = sot223;
EndCmp

BeginCmp
TimeStamp = /5069B48D;
Reference = X1;
ValeurCmp = CRYSTAL;
IdModule  = HC-49V;
EndCmp

EndListe
