(export (version D)
  (design
    (source /home/sebastian/projects/7segment_timer/boards/driver/driverboard.sch)
    (date "Sat 16 Aug 2014 12:04:33 AM CEST")
    (tool "eeschema (2013-may-18)-stable"))
  (components
    (comp (ref J1)
      (value RJ45)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC23CC))
    (comp (ref J2)
      (value RJ45)
      (libsource (lib conn) (part RJ45))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC2875))
    (comp (ref P1)
      (value HE10-10)
      (libsource (lib conn) (part HE10-10))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC2924))
    (comp (ref C3)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC346F))
    (comp (ref C2)
      (value 10uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC348D))
    (comp (ref C5)
      (value 100nF)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC350A))
    (comp (ref C4)
      (value 10uF)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3510))
    (comp (ref R2)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC367C))
    (comp (ref D3)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC36E5))
    (comp (ref R1)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC37A6))
    (comp (ref D1)
      (value LED)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC37AD))
    (comp (ref U1)
      (value 74HC595)
      (libsource (lib 74xx) (part 74HC595))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3814))
    (comp (ref C1)
      (value 100n)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3C4B))
    (comp (ref R10)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC3E80))
    (comp (ref R18)
      (value 470)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC40ED))
    (comp (ref R9)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41BE))
    (comp (ref R17)
      (value 470)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41CB))
    (comp (ref R8)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41D9))
    (comp (ref R16)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41E6))
    (comp (ref R7)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC41F4))
    (comp (ref R15)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4201))
    (comp (ref R6)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC420F))
    (comp (ref R14)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC421C))
    (comp (ref R5)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC422A))
    (comp (ref R13)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4237))
    (comp (ref R4)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4245))
    (comp (ref R12)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4252))
    (comp (ref R3)
      (value 220)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC4260))
    (comp (ref R11)
      (value 160)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52DC426D))
    (comp (ref D2)
      (value BAT42W)
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E410B2))
    (comp (ref U2)
      (value TS2937)
      (libsource (lib ts2937) (part TS2937))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E445FE))
    (comp (ref Q1)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44C4E))
    (comp (ref Q2)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D2E))
    (comp (ref Q3)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D34))
    (comp (ref Q4)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D3A))
    (comp (ref Q5)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D40))
    (comp (ref Q6)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D46))
    (comp (ref Q7)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D4C))
    (comp (ref Q8)
      (value NDS355)
      (libsource (lib nds355) (part NDS355))
      (sheetpath (names /) (tstamps /))
      (tstamp 52E44D52))
    (comp (ref R19)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE823A))
    (comp (ref D4)
      (value ZENER)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8249))
    (comp (ref R20)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8740))
    (comp (ref D5)
      (value ZENER)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8746))
    (comp (ref R21)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE888C))
    (comp (ref D6)
      (value ZENER)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8A44))
    (comp (ref R22)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8B05))
    (comp (ref D7)
      (value ZENER)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8C62))
    (comp (ref R23)
      (value 1k)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8D2A))
    (comp (ref D8)
      (value ZENER)
      (libsource (lib device) (part ZENER))
      (sheetpath (names /) (tstamps /))
      (tstamp 53EE8E6C)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Condensateur polarise")
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part ZENER)
      (description "Diode zener")
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) ZENER)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib conn) (part HE10-10)
      (fields
        (field (name Reference) P)
        (field (name Value) HE10-10)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))
        (pin (num 7) (name 7) (type passive))
        (pin (num 8) (name 8) (type passive))
        (pin (num 9) (name 9) (type passive))
        (pin (num 10) (name 10) (type passive))))
    (libpart (lib conn) (part RJ45)
      (fields
        (field (name Reference) J)
        (field (name Value) RJ45)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name SHIELD) (type passive))))
    (libpart (lib 74xx) (part 74HC595)
      (description "8 bits serial in // out Shift Register 3 State Out")
      (docs 74xx/74HC595.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HC595)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name QB) (type 3state))
        (pin (num 2) (name QC) (type 3state))
        (pin (num 3) (name QD) (type 3state))
        (pin (num 4) (name QE) (type 3state))
        (pin (num 5) (name QF) (type 3state))
        (pin (num 6) (name QG) (type 3state))
        (pin (num 7) (name QH) (type 3state))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name ~QH) (type output))
        (pin (num 10) (name SRCLR) (type input))
        (pin (num 11) (name SRCLK) (type input))
        (pin (num 12) (name RCLK) (type input))
        (pin (num 13) (name G) (type input))
        (pin (num 14) (name SER) (type input))
        (pin (num 15) (name QA) (type 3state))
        (pin (num 16) (name VCC) (type power_in))))
    (libpart (lib nds355) (part NDS355)
      (fields
        (field (name Reference) Q)
        (field (name Value) NDS355)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib ts2937) (part TS2937)
      (fields
        (field (name Reference) U)
        (field (name Value) TS2937)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VI) (type input))
        (pin (num 2) (name GND) (type input))
        (pin (num 3) (name VO) (type power_out)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical 74xx)
      (uri /usr/share/kicad/library/74xx.lib))
    (library (logical nds355)
      (uri ../lib/nds355.lib))
    (library (logical ts2937)
      (uri ../lib/ts2937.lib)))
  (nets
    (net (code 1) (name FET_6)
      (node (ref U1) (pin 5))
      (node (ref R8) (pin 2)))
    (net (code 2) (name SEG_4)
      (node (ref R14) (pin 2))
      (node (ref P1) (pin 8)))
    (net (code 3) (name SEG_3)
      (node (ref P1) (pin 7))
      (node (ref R13) (pin 2)))
    (net (code 4) (name SEG_8)
      (node (ref P1) (pin 4))
      (node (ref R18) (pin 2)))
    (net (code 5) (name SEG_7)
      (node (ref P1) (pin 3))
      (node (ref R17) (pin 2)))
    (net (code 6) (name SEG_6)
      (node (ref R16) (pin 2))
      (node (ref P1) (pin 6)))
    (net (code 7) (name SEG_5)
      (node (ref R15) (pin 2))
      (node (ref P1) (pin 5)))
    (net (code 8) (name SEG_2)
      (node (ref R12) (pin 2))
      (node (ref P1) (pin 10)))
    (net (code 9) (name SEG_1)
      (node (ref P1) (pin 9))
      (node (ref R11) (pin 2)))
    (net (code 10) (name FET_8)
      (node (ref U1) (pin 7))
      (node (ref R10) (pin 2)))
    (net (code 11) (name FET_7)
      (node (ref U1) (pin 6))
      (node (ref R9) (pin 2)))
    (net (code 12) (name FET_5)
      (node (ref U1) (pin 4))
      (node (ref R7) (pin 2)))
    (net (code 13) (name FET_4)
      (node (ref U1) (pin 3))
      (node (ref R6) (pin 2)))
    (net (code 14) (name FET_3)
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 2)))
    (net (code 15) (name FET_2)
      (node (ref R4) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 16) (name FET_1)
      (node (ref R3) (pin 2))
      (node (ref U1) (pin 15)))
    (net (code 17) (name "")
      (node (ref Q4) (pin 2))
      (node (ref R14) (pin 1)))
    (net (code 18) (name "")
      (node (ref Q4) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 19) (name "")
      (node (ref Q3) (pin 2))
      (node (ref R13) (pin 1)))
    (net (code 20) (name "")
      (node (ref Q3) (pin 1))
      (node (ref R5) (pin 1)))
    (net (code 21) (name "")
      (node (ref Q2) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 22) (name "")
      (node (ref R11) (pin 1))
      (node (ref Q1) (pin 2)))
    (net (code 23) (name "")
      (node (ref R3) (pin 1))
      (node (ref Q1) (pin 1)))
    (net (code 24) (name "")
      (node (ref R12) (pin 1))
      (node (ref Q2) (pin 2)))
    (net (code 25) (name "")
      (node (ref Q5) (pin 2))
      (node (ref R15) (pin 1)))
    (net (code 26) (name "")
      (node (ref Q5) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 27) (name "")
      (node (ref Q6) (pin 2))
      (node (ref R16) (pin 1)))
    (net (code 28) (name GND)
      (node (ref C5) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref U1) (pin 13))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 8))
      (node (ref C2) (pin 2))
      (node (ref J1) (pin 9))
      (node (ref J1) (pin 8))
      (node (ref J1) (pin 6))
      (node (ref J2) (pin 6))
      (node (ref J2) (pin 9))
      (node (ref J2) (pin 8))
      (node (ref D8) (pin 1))
      (node (ref D7) (pin 1))
      (node (ref Q8) (pin 3))
      (node (ref Q4) (pin 3))
      (node (ref Q3) (pin 3))
      (node (ref Q2) (pin 3))
      (node (ref Q1) (pin 3))
      (node (ref U2) (pin 2))
      (node (ref D6) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref Q5) (pin 3))
      (node (ref Q6) (pin 3))
      (node (ref Q7) (pin 3))
      (node (ref D4) (pin 1)))
    (net (code 29) (name "")
      (node (ref U1) (pin 10))
      (node (ref R21) (pin 2))
      (node (ref D6) (pin 2)))
    (net (code 30) (name "")
      (node (ref U1) (pin 11))
      (node (ref R20) (pin 2))
      (node (ref D5) (pin 2)))
    (net (code 31) (name "")
      (node (ref R23) (pin 1))
      (node (ref D8) (pin 2))
      (node (ref U1) (pin 9)))
    (net (code 32) (name "")
      (node (ref R19) (pin 2))
      (node (ref D4) (pin 2))
      (node (ref U1) (pin 14)))
    (net (code 33) (name "")
      (node (ref D7) (pin 2))
      (node (ref U1) (pin 12))
      (node (ref R22) (pin 2)))
    (net (code 34) (name "")
      (node (ref Q8) (pin 2))
      (node (ref R18) (pin 1)))
    (net (code 35) (name "")
      (node (ref R10) (pin 1))
      (node (ref Q8) (pin 1)))
    (net (code 36) (name "")
      (node (ref Q7) (pin 2))
      (node (ref R17) (pin 1)))
    (net (code 37) (name "")
      (node (ref R9) (pin 1))
      (node (ref Q7) (pin 1)))
    (net (code 38) (name "")
      (node (ref Q6) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 39) (name +24V)
      (node (ref P1) (pin 1))
      (node (ref D2) (pin 2))
      (node (ref P1) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref C3) (pin 1))
      (node (ref C2) (pin 1)))
    (net (code 40) (name Data_Out)
      (node (ref J2) (pin 5))
      (node (ref R23) (pin 2)))
    (net (code 41) (name Reset)
      (node (ref R21) (pin 1))
      (node (ref J1) (pin 7))
      (node (ref J2) (pin 7)))
    (net (code 42) (name Data_In)
      (node (ref J1) (pin 5))
      (node (ref R19) (pin 1)))
    (net (code 43) (name Enable)
      (node (ref J1) (pin 3))
      (node (ref J2) (pin 3))
      (node (ref R22) (pin 1)))
    (net (code 44) (name Clock)
      (node (ref J1) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref R20) (pin 1)))
    (net (code 45) (name "")
      (node (ref D3) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 46) (name +5V)
      (node (ref U2) (pin 3))
      (node (ref U1) (pin 16))
      (node (ref R2) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 47) (name "")
      (node (ref R1) (pin 2))
      (node (ref D1) (pin 1)))))