Cmp-Mod V01 Created by CvPcb (2013-may-18)-stable date = Tue 19 Aug 2014 08:24:23 PM CEST

BeginCmp
TimeStamp = /52DC3C4B;
Reference = C1;
ValeurCmp = 100n;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC348D;
Reference = C2;
ValeurCmp = 10uF;
IdModule  = c_tant_D;
EndCmp

BeginCmp
TimeStamp = /52DC346F;
Reference = C3;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC3510;
Reference = C4;
ValeurCmp = 10uF;
IdModule  = c_tant_D;
EndCmp

BeginCmp
TimeStamp = /52DC350A;
Reference = C5;
ValeurCmp = 100nF;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC37AD;
Reference = D1;
ValeurCmp = LED;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52E410B2;
Reference = D2;
ValeurCmp = BAT42W;
IdModule  = sod123;
EndCmp

BeginCmp
TimeStamp = /52DC36E5;
Reference = D3;
ValeurCmp = LED;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53EE8249;
Reference = D4;
ValeurCmp = ZENER;
IdModule  = sod123;
EndCmp

BeginCmp
TimeStamp = /53EE8746;
Reference = D5;
ValeurCmp = ZENER;
IdModule  = sod123;
EndCmp

BeginCmp
TimeStamp = /53EE8A44;
Reference = D6;
ValeurCmp = ZENER;
IdModule  = sod123;
EndCmp

BeginCmp
TimeStamp = /53EE8C62;
Reference = D7;
ValeurCmp = ZENER;
IdModule  = sod123;
EndCmp

BeginCmp
TimeStamp = /53EE8E6C;
Reference = D8;
ValeurCmp = ZENER;
IdModule  = sod123;
EndCmp

BeginCmp
TimeStamp = /52DC23CC;
Reference = J1;
ValeurCmp = RJ45;
IdModule  = RJ45_MEBP_8-8G;
EndCmp

BeginCmp
TimeStamp = /52DC2875;
Reference = J2;
ValeurCmp = RJ45;
IdModule  = RJ45_MEBP_8-8G;
EndCmp

BeginCmp
TimeStamp = /52DC2924;
Reference = P1;
ValeurCmp = HE10-10;
IdModule  = HE10-10C;
EndCmp

BeginCmp
TimeStamp = /52E44C4E;
Reference = Q1;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52E44D2E;
Reference = Q2;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52E44D34;
Reference = Q3;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52E44D3A;
Reference = Q4;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52E44D40;
Reference = Q5;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52E44D46;
Reference = Q6;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52E44D4C;
Reference = Q7;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52E44D52;
Reference = Q8;
ValeurCmp = NDS355;
IdModule  = sot23;
EndCmp

BeginCmp
TimeStamp = /52DC37A6;
Reference = R1;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC367C;
Reference = R2;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC4260;
Reference = R3;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC4245;
Reference = R4;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC422A;
Reference = R5;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC420F;
Reference = R6;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC41F4;
Reference = R7;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC41D9;
Reference = R8;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC41BE;
Reference = R9;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC3E80;
Reference = R10;
ValeurCmp = 220;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC426D;
Reference = R11;
ValeurCmp = 160;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /52DC4252;
Reference = R12;
ValeurCmp = 160;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /52DC4237;
Reference = R13;
ValeurCmp = 160;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /52DC421C;
Reference = R14;
ValeurCmp = 160;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /52DC4201;
Reference = R15;
ValeurCmp = 160;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /52DC41E6;
Reference = R16;
ValeurCmp = 160;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /52DC41CB;
Reference = R17;
ValeurCmp = 470;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /52DC40ED;
Reference = R18;
ValeurCmp = 470;
IdModule  = SM1206;
EndCmp

BeginCmp
TimeStamp = /53EE823A;
Reference = R19;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53EE8740;
Reference = R20;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53EE888C;
Reference = R21;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53EE8B05;
Reference = R22;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /53EE8D2A;
Reference = R23;
ValeurCmp = 1k;
IdModule  = SM0603;
EndCmp

BeginCmp
TimeStamp = /52DC3814;
Reference = U1;
ValeurCmp = 74HC595;
IdModule  = SO16E;
EndCmp

BeginCmp
TimeStamp = /52E445FE;
Reference = U2;
ValeurCmp = TS2937;
IdModule  = DPAK2;
EndCmp

EndListe
